December 18, 2024

TMT Coordinated Chum Operation

Bonneville Dam Tailwater for Chum Incubation

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. EFFECTIVE, DECEMBER (INSERT DATE HERE), 2024, AT 0001 HOURS, UNTIL

FURTHER NOTICE, THE BONNEVILLE DAM MINIMUM TAILWATER ELEVATION

IS 11.3 FEET DURING ALL HOURS.