December 18, 2024

TMT Coordinated Chum Operation

Bonneville Dam Tailwater for Chum Incubation

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. EFFECTIVE, DECEMBER (INSERT DATE HERE), 2024, AT 0001 HOURS, UNTIL

FURTHER NOTICE, THE BONNEVILLE DAM MINIMUM TAILWATER ELEVATION

IS 11.3 FEET DURING ALL HOURS.

The operation above was coordinated during the 12/18 TMT meeting. After the meeting additional coordination occurred with WDFW and the coordinated start date was 12/19 at 1pm.